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Specification


Lamp options: 


3 x 14W T5


4 x 14W T5


Slimline steel body.


Welded corners for added rigidity


White polyester powder-paint finish - RAL9010.


High frequency gear as standard or regulating control gear option.


Luminaire sits on ceiling tee or pulls up from below, using optional side support brackets.


Fitting depth 61mm


Installation depth 150mm (lay-in)


61mm installation depth using side support brackets


Air Handling 25l/s








Louvre


Highly reflective (95%), zero iridescence Miro 4 Cat2.200.


Positive spring retention.


Full perimeter flange reduces light spill.


Closed top wedge.
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